## succbone
succbone is our "automation" system for the vacuum system of the SEM.

![succbone control panel](./succbone-control-panel.jpg)

### Features
- Read a TPR280 pirani gauge (0-10V analog input)
- 8x relay outputs for
  - Roughing pump interlock
  - Diffusion pump interlock
  - Emulate _Pump-Down_ push button
  - Emulate _Vent_ push button
  - Signal two different vacuum levels to the original evacuation controller
    * Rough vacuum reached
    * High vacuum reached
